Monitoring & Management

BM-SM and BM-GW collect sensor data for visualization via HTTP interface or HMI. Users can monitor all battery metrics in real-time, configure thresholds, and manage system behavior.

BM-GW WEB UI

Demo: BTMS BM-GW WEB UI demo

User: demo

Pass: demo

Log-in

1st time log in:

Connect Ethernet 2 port to facility LAN

Connect PC to Ethernet 1 port (standard Ethernet cable between PC and BM-GW Ethernet 1 port)

For PC Ethernet connection set fixed IP 192.168.10.200.

Use the Internet browser to go to https://192.168.10.1

Log in as:

user: admin

password: bmgw!admin

Check the WAN IP address on the Data center - Settings page and set it if necessary

Connect the PC to the facility LAN and go to the https://IP address of the WAN port

General description

1	Pages tabs
2	Data center tree structure
3	Page data

Data center

Real-time data

1	Tabular display of data for the Data Center
2	Select a parameter for the graphic display
3	Graphic bar-graph data display for the data center

Discharge data

1	Discharge events table
2	String time-plot for discharge event
3	Cell time-plot for discharge event

String time-plot for discharge event

Cell time-plot for discharge event

1	Cell selection

Alarm

1	Alarms sub-page selection
2	Alarms table

E-mails

SMS

Settings

Network settings, NTP settings

Time settings, Users

SNMP settings, SMS notifications, Project settings, Data export

UPS

Real-time data

History data

Discharge data

String time-plot

Cell time-plot

Alarm

String

Real-time data

String

Cells

History data

String

Cells

Discharge data

String time-plot

Cell time-plot

Alarm

Settings

Enable for which alarm SMS / e-mail will be sent.